**HOW TO SETUP SFTP CONNECTION IN HCI TENANT**

1. Get the *SFTP Server* details


**SF SFTP Server Test Details**

URL: sftp4.successfactors.com


Username: 163030T


Password: \*\*\*\*\*\*\*\*

1. Go to *Manage Security Material* in the *Monitoring Page* (eye icon) of HCI tenant




1. Deploy the SFTP Credential. Click *Add* then *User Credentials*







1. Go to *Connectivity Tests* in the *Monitoring Page* of HCI tenant




1. Test the connection of the SFTP following the below setup then click *Send*.




1. After clicking the Send button, you will see the response details at the right. Click *Copy Host Key*.




1. Paste the Host Key in notepad. Put a note or name of the SFTP in the first line then the Host Key. Put a # sign before the name to indicate that part as a comment. See sample:




1. Save the file as known\_hosts (without any file extension)




1. Go back to *Manage Security Material* and deploy the known\_hosts file. Click *Add SSH Known Hosts*






1. Go back to Connectivity Tests. Check the SFTP Connectivity using the User Credential deployed in Step 3. Follow below setup:



**MULTIPLE SFTP SERVERS IN ONE KNOWN HOST FILE**

1. Edit the known\_hosts file. Separating each SFTP host key. See sample below:



1. Save the updated file.
2. Redeploy the known\_hosts using the updated file.